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Call for Comments to the Proposed General Amendments to the WESM Rules and Various WESM Manuals on Forecast Accuracy Standards for Scheduled VREs
(ORCP- WR-WM-26-06)

The Rules Change Committee (RCC) is inviting all WESM Members and interested parties to submit comments to Proposed General Amendments to the WESM Rules and Various WESM Manuals on Forecast Accuracy Standards for Scheduled VREs (ORCP- WR-WM-26-06).

The Proponent, ACEN Corporation, seeks to amend the WESM Rules and various WESM Manuals to:

· Apply Forecast Accuracy Standards (FAS), in lieu of Dispatch Conformance Standards (DCS), to Variable Renewable Energy (VRE) generating units that elect to operate as Scheduled Generating Units;
· Enable offer-based participation and greater responsiveness of VRE generators to market price signals;
· Allow VRE generators to manage exposure to negative prices and reduce uneconomic dispatch;
· Maintain forecast accountability through the existing FAS framework; and
· Implement the necessary amendments to the WESM Rules and relevant WESM Manuals to give effect to the proposed changes.

 The WESM document/s for amendment are the following:
1. WESM Rules
1. Dispatch Protocol (WESM-DP), Issue 25.0
1. Procedures for the Monitoring of Forecast Accuracy Standards for Must-Dispatch Generating Units (WESM-FASMD), Issue 3.0
1. Registration Manual (WESM-RSDCP), Issue 18.0


BACKGROUND:

The ACEN Corporation submitted the proposed amendments on 08 September 2026 as an Urgent Amendment. Upon deliberation during its 262nd Regular Meeting, the RCC determined that the proposal did not meet the urgency criteria and subsequently reclassified it as a General Amendment proposal. Consequently, the PEM Board, during its 100th Meeting on 30 September 2026, concurred with the RCC’s decision on the said proposal.






DOCUMENTS:

 Provided below are relevant materials for your reference and perusal: 
· Original Rules Change Proposal (Urgent Amendment) submitted by ACEN Corporation (ORCP-WR-WM-26-05)
· Presentation of the Proposed Amendments
· RCC decision to reclassify the proposal as General Amendment (RCC Resolution No. 2026-06)
· RCC Form3_Matrix of Proposed Amendments for Comments - Annexes of this document (Please write your comments in the proper columns in the matrix.)
 
Kindly submit your comments (in Word format) through the File a Submission webpage no later than 20 November 2026 or 30 working days from the date of publication (05 October 2026). We recommend using Firefox browser for submitting your comments. 

Please ensure that your submission is signed securely by the designated approving authority and/or representative of your company, and input in the proper field the e-mail address of your point person(s) whom we could contact regarding activities related to the processing of the proposal. All comments received shall be published in the PEMC website.

Thank you!



TO BE ACCOMPLISHED BY THE PARTY SUBMITTING THE COMMENTS

[In accomplishing and submitting this form, you give your consent for PEMC to collect, record, organize, and update your personal data as herein provided as part of your information for purposes of rules change process.]

Commenter’s Information 

	Name 
	
[Signature over Name]

	Designation         
	

	Company              
	

	Company Address               
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Comments to the  Proposed General Amendments to the WESM Rules and Various WESM Manuals on Forecast Accuracy Standards for Scheduled VREs

	Commenter
	General Comments
	Proponent’s Response

	
	Please write your general comment here, if any:
	



	WESM Rules (as of 31 August 2025)

	Title
	Section
	Provision
	Proposed Amendment
	Rationale
	Comments
	Proposed Wording based on Comments
	Original Proponent’s Response
	RCC Decision

	2.3 CATEGORIES OF WESM MEMBER

2.3.1 Generation Company
	2.3.1.8
	A Generation Company is required to operate scheduled generating units and priority dispatch generating units in accordance with the scheduling and dispatch procedures described in Chapter 3, and in accordance with the dispatch conformance standards specified in accordance with Clause 3.8.5.
	A Generation Company is required to operate scheduled generating units and priority dispatch generating units in accordance with the scheduling and dispatch procedures described in Chapter 3, and in accordance with the dispatch conformance standards specified in accordance with Clause 3.8.5. Intermittent Renewable Energy Resource-based generating unit that opt to be classified as a scheduled generating unit shall comply with forecast accuracy standards in accordance with the relevant Market Manual in lieu of the dispatch conformance standards.
	Clause 2.3.1.8 imposes DCS on all scheduled generating units without exception. The provision carves out VREs or Intermittent RE Resources opting to be classified as scheduled generators and directs their compliance to FAS under the relevant Market Manual, consistent with the primary amendment in DPM Section 12.4.1(e), in lieu of DCS.
	
	
	
	

	3.5.5 Generation Offers and Data
	3.5.5.11
	A Trading Participant who fails to meet the requisite forecast accuracy standards set out in accordance with Clause 3.5.5.9, based on the results of an annual assessment, shall be liable for sanctions imposed under Clause 7.2 and the WESM Penalty Manual.
	A Trading Participant who fails to meet the requisite forecast accuracy standards set out in accordance with Clause 3.5.5.9 or Clause 3.5.5.15, based on the results of an annual assessment, shall be liable for sanctions imposed under Clause 7.2 and the WESM Penalty Manual.
	Sanction trigger extended to cover FAS non-compliance by Intermittent Renewable Energy Resource that opted to be classified as a scheduled generating unit under new Clause 3.5.5.15.
	
	
	
	

	3.5.5 Generation Offers and Data
	3.5.5.12
	The Enforcement and Compliance Office shall report to the PEM Board, the Compliance Committee, the ERC, and the DOE the monthly and annual compliance of each must-dispatch generating unit to the forecast accuracy standards with respect to its projected outputs.
	The Enforcement and Compliance Office shall report to the PEM Board, the Compliance Committee, the ERC, and the DOE the monthly and annual compliance of each must-dispatch generating unit to the forecast accuracy standards with respect to its projected outputs. For an intermittent renewable energy resource‑based generating unit that has opted to be classified as scheduled generating unit, the last tranche of the market offer shall be equal to its projected output.
	ECO’s reporting obligation has been extended to Intermittent Renewable Energy Resource that opted to be classified as a scheduled generating unit.

The reference to projected outputs have been updated to include market offers as the applicable submission input for Intermittent Renewable Energy Resource that opted to be classified as a scheduled generating unit, provided that the last tranche of the offer shall be equal to its projected output.
	
	
	
	

	3.5.5 Generation Offers and Data
	3.5.5.15 
	[Proposed New provision. Parent provision shown for reference:]

Parent provision — Clause 3.5.5.9:
Must-dispatch generating units shall comply with forecast accuracy standards, in respect of their projected outputs submitted under Clause 3.5.5.6, consistent with the Grid Code.
	Intermittent Renewable Energy Resource-based generating unit that opt to be classified as a scheduled generating unit shall comply with forecast accuracy standards, in respect of their projected output submitted under Clause 3.5.5.6, in accordance with the relevant Market Manuals and consistent with the provisions of the Grid Code.
	New clause establishing forecast accuracy standards (FAS) as the applicable compliance standard for Intermittent Renewable Energy Resource that opted to be classified as a scheduled generating unit. 

This is a parallel structure to Clause 3.5.5.9 for must-dispatch units, Intermittent Renewable Energy Resource that opted to be classified as a scheduled generating unit submit its projected output under Clause 3.5.5.6.
	
	
	
	

	3.5.5 Generation Offers and Data
	3.5.5.16 
	[Proposed New provision. Parent provision shown for reference:]

Parent provision — Clause 3.5.5.10:
The Enforcement and Compliance Office shall evaluate annually the forecast accuracy standards complied with by must-dispatch generating units in accordance with Clause 3.5.5.9.
	The Enforcement and Compliance Office shall evaluate annually the forecast accuracy standards complied with by Intermittent Renewable Energy Resource-based generating unit that opt to be classified as a scheduled generating unit in accordance with Clause 3.5.5.15.
	The annual evaluation by the Enforcement and Compliance Office (ECO) is extended to Intermittent Renewable Energy Resource that opted to be classified as a scheduled generating unit under new Clause 3.5.5.15.
	
	
	
	

	GLOSSARY

	Chapter 11 
	Dispatch Conformance Standards. Standards that set the criteria and procedures for determining whether the scheduled generating units and the priority dispatch generating units comply with their dispatch schedules and which are required to be set out in a Market Manual in accordance with Clause 3.8.5.
	Dispatch Conformance Standards. Standards that set the criteria and procedures for determining whether the scheduled generating units and the priority dispatch generating units comply with their dispatch schedules and which are required to be set out in a Market Manual in accordance with Clause 3.8.5. Intermittent renewable energy resource‑based generating units that opt to be classified as scheduled generating units pursuant to the WESM Rules, shall comply with forecast accuracy standards in accordance with the relevant Market Manuals, in lieu of the dispatch conformance standards, and the last tranche of the market offer shall be equal to its projected output.
	The definition contains an implicit population scope that, without a clarifying sentence, would be read as applying to all scheduled generating units. The addition flags the exemption of VREs classified as scheduled generators to prevent interpretive ambiguity at the definition level.
	
	
	
	

	GLOSSARY
	Chapter 11
	(New)
	Forecast Accuracy Standards. Standards that set the criteria and procedures for determining whether the must dispatch generating units and the Intermittent Renewable Energy Resource-based generating unit that opted to be classified as a scheduled generating units comply with the submission to the Market Operator of their projected outputs, which are required to be set out in a Market Manual. For an intermittent renewable energy resource‑based generating unit that has opted to be classified as scheduled generating unit, the last tranche of the market offer shall be equal to its projected output.
	FAS has not been defined in the Rules and in any of the Market Manuals. This proposal is to streamline reference to Forecast Accuracy Standards in the existing Rules and the proposed amendments.
	
	
	
	




	Dispatch Protocol Manual (WESM-DP), Issue 25.0 (as of 11 April 2026)

	Title
	Section
	Provision
	Proposed Amendment
	Rationale
	Comments
	Proposed Wording based on Comments
	Original Proponent’s Response
	RCC Decision

	Section 12 Dispatch Compliance

12.1 Background
	12.1.1
	A Generation Company is required to operate their scheduled generating units and/or priority dispatch generating units in accordance with the scheduling and dispatch procedures described in Chapter 3 of the WESM Rules. More specifically, scheduled generating units and priority dispatch generating units shall generate in accordance with the dispatch schedules communicated pursuant to WESM Rules Clause 3.8.1 and in accordance with the dispatch conformance standards specified in Clause 3.8.5. They are to follow such schedules unless otherwise restricted or instructed by the System Operator.
	A Generation Company is required to operate their scheduled generating units and/or priority dispatch generating units in accordance with the scheduling and dispatch procedures described in Chapter 3 of the WESM Rules. More specifically, scheduled generating units and priority dispatch generating units shall generate in accordance with the dispatch schedules communicated pursuant to WESM Rules Clause 3.8.1 and in accordance with the dispatch conformance standards specified in Clause 3.8.5. They are to follow such schedules unless otherwise restricted or instructed by the System Operator. Intermittent renewable energy resource-based generating units that opt to be classified as a scheduled generating unit shall comply with forecast accuracy standards in accordance with the relevant Market Manuals in lieu of the dispatch conformance standards.
	General provision updated to reflect that Intermittent Renewable Energy Resource-based generating units that opt to be classified as a scheduled generating unit are not subject to DCS. The qualifying sentence is added at the end of the existing paragraph to avoid restructuring the section.
	
	
	
	

	Section 12 Dispatch Compliance

12.2 Scope and Purpose
	12.2.5. (New)
	[Proposed New provision. Parent provision shown for reference:]

Parent provision — Section 12.2.2:
For scheduled generating units and priority dispatch generating units, this Section establishes the dispatch conformance standards and procedures for monitoring compliance that are required to be established and be set out in a Market Manual pursuant to WESM Rules Clause 3.8.5.
	12.2.5. This Section does not apply to Intermittent RE resource‑based generating units that opt to be classified as scheduled generating units pursuant to the WESM Rules, and that are governed by forecast accuracy standards in accordance with the relevant Market Manuals.
	New section inserted immediately after Section 12.2. to explicitly exclude VREs classified as scheduled generators from the scope of the DCS monitoring regime in Section 12. Without this provision, Section 12.2.3 — which states that this Section applies to all Trading Participants registered as Generation Companies — would override the amendment by bringing VREs as scheduled within DCS scope.
	
	
	
	

	12.3 Responsibilities
	12.3.2 (b)
	The Market Operator is responsible for: 
(a) Coordinating with the System Operator for the periodic review of the dispatch conformance standards as well as of the procedures set out in this Section; and 
(b) Providing a mechanism for monitoring and for notifying Trading Participants of possible breach by scheduled generating units and priority dispatch generating units with the dispatch conformance standards.
	The Market Operator is responsible for: 
(a) Coordinating with the System Operator for the periodic review of the dispatch conformance standards as well as of the procedures set out in this Section; and 
(b) Providing a mechanism for monitoring and for notifying Trading Participants of possible breach by scheduled generating units (except intermittent renewable energy resource‑based generating units that opt to be classified as scheduled generating units pursuant to the WESM Rules) and priority dispatch generating units with the dispatch conformance standards.
	Without this carve-out, VREs which opt to be classified as scheduled generators will be covered by DCS and the MO's DCS monitoring mechanism would apply to them, generating erroneous breach flags. As proposed, their compliance will be monitored under FAS procedures in the WESM-FASMD, not under this DCS mechanism.
	
	
	
	

	12.4 Compliance with Dispatch Schedules and Instructions

12.4.1 Compliance by the Scheduled Generating Units and Priority Dispatch Generating Units.
	12.4.1(a)
	12.4.1 xxx

a. All scheduled generating units and priority dispatch generating units shall comply with their respective dispatch schedules. This obligation shall also apply to the scheduled generating units and priority dispatch generating units with a Final Certificate of Approval to Connect but with pending issuance of the Certificate of Compliance from the ERC. In complying with their dispatch schedules, said generating units shall generate in accordance with the dispatch conformance standards prescribed in Section 12.5 of the Dispatch Protocol. In the case of a priority dispatch generating unit, compliance with the dispatch conformance standards shall also apply in cases where its dispatch schedule was restricted pursuant to WESM Rules Clauses 3.6.1.7 and 3.6.1.8 because of a potential system security contingency. 

xxx

	12.4.1 xxx

a. All scheduled generating units and priority dispatch generating units shall comply with their respective dispatch schedules, except as provided in Section 12.4.1(e). This obligation shall also apply to the scheduled generating units and priority dispatch generating units with a Final Certificate of Approval to Connect but with pending issuance of the Certificate of Compliance from the ERC. In complying with their dispatch schedules, said generating units shall generate in accordance with the dispatch conformance standards prescribed in Section 12.5 of the Dispatch Protocol. In the case of a priority dispatch generating unit, compliance with the dispatch conformance standards shall also apply in cases where its dispatch schedule was restricted pursuant to WESM Rules Clauses 3.6.1.7 and 3.6.1.8 because of a potential system security contingency.

xxx
	Minimal addition: a cross-reference to new Section 12.4.1(e) inserted at the end of the first sentence. This is sufficient to direct participants to the carve-out provision without restructuring the existing obligation.
	
	
	
	

	12.4 Compliance with Dispatch Schedules and Instructions

12.4.1 Compliance by the Scheduled Generating Units and Priority Dispatch Generating Units.
	12.4.1(e) (New)
	[Proposed New provision. Parent provision shown for reference:]
Parent provision — Section 12.4.1 (header and sub-clause (a)):

Compliance by the Scheduled Generating Units and Priority Dispatch Generating Units. 

All scheduled generating units and priority dispatch generating units shall comply with their respective dispatch schedules.... xxx
	Notwithstanding Section 12.4.1(a), Intermittent RE resource‑based generating units that opted to be classified as scheduled generating units pursuant to the WESM Rules shall comply with forecast accuracy standards in accordance with the relevant Market Manuals, in lieu of the dispatch conformance standards.
	This is the primary operative DPM amendment. 
New sub-clause inserted under Section 12.4.1 establishing FAS as the applicable compliance standard for VREs classified as scheduled generators. Maintained as a sub-clause within 12.4.1 to preserve the structural parallel with existing compliance sub-clauses by generator type.
	
	
	
	

	12.5 Dispatch Conformance Standards

12.5.1 Dispatch Compliance Criteria
	12.5.1(b)
	12.5.1 Dispatch Compliance Criteria 
a. xxx

b. All scheduled and priority dispatch generating units shall not deviate beyond the upper and lower dispatch thresholds of +1.5% or -3% of the dispatch schedule or +/-1MW, whichever is higher, as follows: 
 xxx
	12.5.1 Dispatch Compliance Criteria 
a. xxx

b. All scheduled and priority dispatch generating units shall not deviate beyond the upper and lower dispatch thresholds of +1.5% or -3% of the dispatch schedule or +/-1MW, whichever is higher, as follows: 
 xxx

This Section shall not apply to intermittent RE resource‑based generating units that opted to be classified as scheduled generating units pursuant to the WESM Rules.

	Carve-out added to exclude VREs that opted to be classified as scheduled generators from the +1.5%/-3% DCS threshold. VREs as scheduled are assessed under FAS (MAPE/Perc95) pursuant to proposed new Section 12.4.1(e) above.
	
	
	
	

	12.5 Dispatch Conformance Standards

12.5.2 Detection of Non-Compliance and Possible Breach
	12.5.2(a)
	a. Scheduled generating units and priority dispatch generating units shall be flagged for non-compliance with dispatch schedules and for possible breach of the dispatch conformance standards. 

xxx
	a. Scheduled generating units and priority dispatch generating units shall be flagged for non-compliance with dispatch schedules and for possible breach of the dispatch conformance standards. Intermittent renewable energy resource‑based generating units that opted to be classified as scheduled generating units pursuant to the WESM Rules shall not be flagged for non-compliance under this Section.

xxx
	VREs classified as scheduled generators shall be excluded from DCS non-compliance flagging. Their compliance is monitored under FAS procedures in the WESM-FASMD. This prevents erroneous breach flags for conduct that VREs as scheduled are not required to conform to.
	
	
	
	








	Registration, Suspension and De-Registration Criteria and Procedures (WESM-RSDCP), Issue 18.0 (as of 13 February 2024)

	Title
	Section
	Provision
	Proposed Amendment
	Rationale
	Comments
	Proposed Wording based on Comments
	Original Proponent’s Response
	RCC Decision

	2.5.4. Other Considerations

2.5.4.3 Dispatch Conformance Standards
	2.5.4.3
	A Generation Company shall operate scheduled generating units, priority dispatch generating units, battery energy storage systems and pumped-storage units in accordance with the scheduling and dispatch procedures described in Chapter 3, and in accordance with the dispatch conformance standards specified in accordance with Clause 3.8.5.

	A Generation Company shall operate scheduled generating units, priority dispatch generating units, battery energy storage systems and pumped-storage units in accordance with the scheduling and dispatch procedures described in Chapter 3, and in accordance with the dispatch conformance standards specified in accordance with Clause 3.8.5. Notwithstanding anything to the contrary in this Market Manual, including Sections 2.5.4 and 2.5.7, intermittent renewable energy resource‑based generating units that have opted to be classified as scheduled generating units pursuant to the WESM Rules shall not be subject to the Dispatch Conformance Standards. 
	RSDCP-level DCS mandate mirrors WESM Rules Clause 2.3.1.8. Proviso added consistent with WESM Rules and DPM amendments to carve out VREs classified as scheduled generators.
	
	
	
	

	2.5.7. Approval of Applications

2.5.7.3. Guidelines for Test and Commissioning Registration
	2.5.7.3 (b) (i)
	xxx

b) For  its  must-dispatch  generating  units, the  Generation Company shall submit projected output to the Market Operator and comply with the applicable forecast accuracy standards; and

	xxx

b) For its must-dispatch generating units, the Generation Company shall submit projected output to the Market Operator and comply with the applicable forecast accuracy standards. For an intermittent renewable energy resource‑based generating unit that has opted to be classified as scheduled generating unit, the last tranche of the market offer shall be equal to its projected output; and
	Sub-item (i) is the FAS track during FCATC/COC-pending status. Extended to include VREs classified as scheduled generators, who comply with FAS via market offer submission rather than projected output.
	
	
	
	





	Procedures for the Monitoring of Forecast Accuracy Standards (WESM-FASMD), Issue 3.0 (as of 8 February 2024)

	Title
	Section
	Provision
	Proposed Amendment
	Rationale
	Comments
	Proposed Wording based on Comments
	Original Proponent’s Response
	RCC Decision

	1.1 Background
	1.1.1
	The WESM Rules requires generation companies to submit to the Market Operator projected outputs in respect of their must-dispatch generating units for each dispatch interval.
	The WESM Rules requires generation companies to submit to the Market Operator projected outputs in respect of their must-dispatch generating units, for each dispatch interval. For an intermittent renewable energy resource‑based generating unit that has opted to be classified as scheduled generating unit, the last tranche of the market offer shall be equal to its projected output.

	Extended to cover VREs classified as scheduled generators. For must-dispatch units, the relevant submission is projected outputs.  For VREs as scheduled, the submission is market offers under Clause 3.5.5.1 — stated within the clause to preserve accuracy of the cited obligation type.
	
	
	
	

	1.1 Background
	1.1.2
	Consistent with the Grid Code, the WESM Rules also requires must-dispatch generating units to comply with forecast accuracy standards in respect of their projected outputs.
	Consistent with the Grid Code, the WESM Rules also requires must-dispatch generating units, to comply with forecast accuracy standards in respect of their projected. For an intermittent renewable energy resource‑based generating unit that has opted to be classified as scheduled generating unit, the last tranche of the market offer shall be equal to its projected output.

	Extended to cover VREs that opted to be classified as scheduled generators. Reference to projected outputs supplemented with market offers, consistent with the distinct submission mechanism applicable to VREs as scheduled.
	
	
	
	

	1.1 Background
	1.1.3
	A Generation Company that has secured a Final Certificate of Approval to Connect for completing the conduct of test and commissioning but with pending issuance of Certificate of Compliance from the ERC for its must- dispatch generating unit shall comply with the forecast accuracy standards in respect of its projected outputs.
	A Generation Company that has secured a Final Certificate of Approval to Connect for completing the conduct of test and commissioning but with pending issuance of Certificate of Compliance from the ERC for its must- dispatch generating unit, shall comply with the forecast accuracy standards in respect of its projected outputs. For an intermittent renewable energy resource‑based generating unit that has opted to be classified as scheduled generating unit, the last tranche of the market offer shall be equal to its projected output.

	Extended to cover VREs that opted to be classified as scheduled generators in FCATC/COC-pending status, consistent with the RSDCP Section 2.5.7.3(b)(i) amendments.
	
	
	
	

	1.1 Background
	1.1.6
	The Enforcement and Compliance Office shall report to the PEM Board, the Compliance Committee, the ERC, and the DOE the annual compliance of each must-dispatch generating unit to the forecast accuracy standards with respect to its projected outputs.
	The Enforcement and Compliance Office shall report to the PEM Board, the Compliance Committee, the ERC, and the DOE the annual compliance of each must-dispatch generating unit to the forecast accuracy standards with respect to its projected outputs. For an intermittent renewable energy resource‑based generating unit that has opted to be classified as scheduled generating unit, the last tranche of the market offer shall be equal to its projected output.
	Extended to cover VREs that opted to be classified as scheduled generators. Reference to projected outputs supplemented with market offers.
	
	
	
	

	1.2 Purpose
	1.2.1
	This Market Manual shall establish the forecast accuracy standards that must-dispatch generating units are required to comply with.
	This Market Manual shall establish the forecast accuracy standards that must-dispatch generating units or intermittent renewable energy resource‑based generating units that opted to be classified as scheduled generating units are required to comply with.
	Purpose statement extended to cover VREs that opted to be classified as scheduled generators.
	
	
	
	

	1.2 Purpose
	1.2.2
	This Market Manual shall provide the equations that will be used in determining the compliance of must-dispatch generating units with the forecast accuracy standards.
	This Market Manual shall provide the equations that will be used in determining the compliance of must-dispatch generating units or an intermittent renewable energy resource‑based generating units that opted to be classified as scheduled generating unit with the forecast accuracy standards.
	Purpose statement extended to cover VREs that opted to be classified as scheduled generators.
	
	
	
	

	1.2 Purpose
	1.2.3
	This Market Manual shall specify the procedures for the monitoring and reporting of the compliance of must-dispatch generating units with the forecast accuracy standards.
	This Market Manual shall specify the procedures for the monitoring and reporting of the compliance of must-dispatch generating units or intermittent renewable energy resource‑based generating units that opted to be classified as scheduled generating units with the forecast accuracy standards.
	Purpose statement extended to cover VREs that opted to be classified as scheduled generators.
	
	
	
	

	1.3 Scope
	1.3.1
	This Market Manual only provides the standards and procedures for must-dispatch generating units registered in the WESM.
	This Market Manual only provides the standards and procedures for must-dispatch generating units and intermittent renewable energy resource‑based generating units that opted to be classified as scheduled generating units registered in the WESM.
	Scope extended to include VREs that opted to be classified as scheduled generators as the second population subject to FAS monitoring.
	
	
	
	

	1.3 Scope
	1.3.3 (New)
	(New)
	The provisions of this Market Manual in respect of “must‑dispatch generating units,” shall likewise apply to intermittent renewable energy resource‑based generating units that opted to be classified as Scheduled Generating Units pursuant to the WESM Rules, unless the context clearly indicates otherwise. 

	Extended to cover VREs that opted to be classified as scheduled generators, ensuring expansion capacity of VREs that have elected scheduled status.

· Including 2.1.2(a) on the Expansion Unit

	
	
	
	

	2.1 Definition 
	2.1.2(a)
	a) Expansion Unit. It shall refer to the expanded capacity of a must-dispatch generating unit which may be built in phases and designed to utilize the same plant substation and revenue meter being used by the existing capacity unit. 

	a) Expansion Unit. It shall refer to the expanded capacity of a must-dispatch generating unit or an intermittent renewable energy resource‑based generating unit that opted to be classified as scheduled generating unit which may be built in phases and designed to utilize the same plant substation and revenue meter being used by the existing capacity unit.
	Extended to cover VREs that opted to be classified as scheduled generators, ensuring expansion capacity of VREs that have elected scheduled status is treated consistently under Section 4.2.8.
	
	
	
	

	2.1 Definition
	2.1.2(c)
	c) Forecast Percentage Error (FPE). Error (in %) of the projected output submitted by a must-dispatch generating unit with respect to its maximum metered quantity over a billing period as dependable capacity and calculated in accordance with Section 4.2.3. 

	c) Forecast Percentage Error (FPE). Error (in %) of the projected output submitted by a must-dispatch generating unit, with respect to its maximum metered quantity over a billing period as dependable capacity and calculated in accordance with Section 4.2.3. For an intermittent renewable energy resource‑based generating unit that has opted to be classified as scheduled generating unit, RTD Schedule shall replace the projected output.
	FPE definition extended to cover VREs that opted to be classified as scheduled generators. Without this update, FPE — and therefore MAPE and Perc95 — cannot be validly calculated for VREs as scheduled, rendering the FAS obligation unenforceable. The definition carries through all provisions that reference FPE, including Sections 4.2.1, 4.2.2, 4.2.3, 4.2.5, 4.2.6, and 4.2.7 where the projected output shall be equal to the RTD Schedule.
	
	
	
	

	2.1 Definition
	2.1.2(e)
	e) Mean Absolute Percentage Error (MAPE). Mean of the forecast percentage errors of a must-dispatch generating unit over a certain period calculated in accordance with Section 4.2.1. 

	e) Mean Absolute Percentage Error (MAPE). Mean of the forecast percentage errors of a must-dispatch generating unit or an intermittent renewable energy resource‑based generating unit that opted to be classified as scheduled generating unit over a certain period calculated in accordance with Section 4.2.1.
	Extended to cover VREs classified as scheduled generators. MAPE is derived from FPE values, which are themselves extended via the amended FPE definition.
	
	
	
	

	2.1 Definition
	2.1.2(g)
	g) Projected quantity. Estimated generation of a must-dispatch generating unit over a dispatch interval based on its submitted projected output assuming linear ramping calculated in accordance with Section 4.2.4. 

	g) Projected quantity. Estimated generation of a must-dispatch generating unit over a dispatch interval based on its submitted projected output assuming linear ramping calculated in accordance with Section 4.2.4. For an intermittent renewable energy resource‑based generating unit that has opted to be classified as scheduled generating unit, RTD Schedule shall replace the projected output.
	Redefined to cover both populations. The distinction between projected output (must-dispatch) and offered quantity (VREs as scheduled) is stated within the definition. This single redefinition carries through all provisions referencing Projected Quantity, including Sections 4.2.3, 4.2.5, 4.2.6, and 4.2.7, eliminating the need for separate formula sub-clauses.
	
	
	
	

	3.1 Enforcement and Compliance Office
	3.1.1
	The Enforcement and Compliance Office shall assess, evaluate, and issue the cumulative results of MAPE and PERC95 to each must-dispatch generating unit on a monthly and annual basis in accordance with the procedures set forth in Section 4.4 hereof. 

The Enforcement and Compliance Office shall, for this purpose, establish a detailed process or procedure of compliance monitoring and assessment and prescribe a reply format or template that may be accomplished by the Generation Company as part of the monitoring process.
	The Enforcement and Compliance Office shall assess, evaluate, and issue the cumulative results of MAPE and PERC95 to each must-dispatch generating unit or intermittent renewable energy resource‑based generating unit that opted to be classified as scheduled generating unit on a monthly and annual basis in accordance with the procedures set forth in Section 4.4 hereof. 

The Enforcement and Compliance Office shall, for this purpose, establish a detailed process or procedure of compliance monitoring and assessment and prescribe a reply format or template that may be accomplished by the Generation Company as part of the monitoring process.
	ECO assessment obligation extended to VREs that opted to be classified as scheduled generators.
	
	
	
	

	3.1 Enforcement and Compliance Office 
	3.1.2
	The Enforcement and Compliance Office shall report to the PEM Board, the Compliance Committee, the ERC, and the DOE its evaluation on the annual compliance of each must-dispatch generating unit to the forecast accuracy standards as set forth in Section 4.4.6 of this Manual.
	The Enforcement and Compliance Office shall report to the PEM Board, the Compliance Committee, the ERC, and the DOE its evaluation on the annual compliance of each must-dispatch generating unit or intermittent renewable energy resource‑based generating unit that opted to be classified as scheduled generating unit to the forecast accuracy standards as set forth in Section 4.4.6 of this Manual.
	ECO reporting obligation extended to VREs that opted to be classified as scheduled generators.
	
	
	
	

	3.2 System Operator
	3.2.1
	The System Operator shall advise the Market Operator of any output restrictions imposed by the System Operator on must-dispatch generating units in accordance with the WESM Rules and the Grid Code.
	The System Operator shall advise the Market Operator of any output restrictions imposed by the System Operator on must-dispatch generating unit or intermittent renewable energy resource‑based generating unit that opted to be classified as scheduled generating unit in accordance with the WESM Rules and the Grid Code.
	Extended to VREs that opted to be classified as scheduled generators. SO output restriction advisory is relevant to both populations for purposes of the exclusion provisions under Section 4.3(b).
	
	
	
	

	3.3 Metering Services Providers 
	3.3.1
	Metering Services Providers of must-dispatch generating units shall submit settlement-ready metering data of must-dispatch generating units in accordance with the timeline provided in the relevant Market Manual.
	Metering Services Providers of must-dispatch generating unit or intermittent renewable energy resource‑based generating unit that opted to be classified as scheduled generating unit shall submit settlement-ready metering data of must-dispatch such generating units in accordance with the timeline provided in the relevant Market Manual.
	MSP data submission obligation extended to VREs that opted to be classified as scheduled generators. Metered quantity data is required for FPE calculation for both populations.
	
	
	
	

	3.4 Generation Companies 
	3.4.1
	Generation companies shall comply with the forecast accuracy standards in this Market Manual in respect of the projected outputs of their must-dispatch generating units submitted in accordance with the WESM Rules.
	Generation companies shall comply with the forecast accuracy standards in this Market Manual in respect of the projected outputs of their must-dispatch generating units, submitted in accordance with the WESM Rules. For an intermittent renewable energy resource‑based generating unit that has opted to be classified as scheduled generating unit, the last tranche of the market offer shall be equal to its projected output.
	GenCo FAS compliance obligation extended to VREs that opted to be classified as scheduled generators. Market offers are identified as the relevant submission input for VREs as scheduled.
	
	
	
	

	3.5 Market Operator 
	3.5.2
	The Market Operator shall provide to the Enforcement and Compliance Office all the market data and information, including the System Operator-validated individual and aggregated forecast data, necessary for the calculation of MAPE and PERC95 and for verification or validation of data, when necessary.
	The Market Operator shall provide to the Enforcement and Compliance Office all the market data and information, including the System Operator-validated individual and aggregated forecast data and RTD schedule and actual dispatch or metered quantity for an intermittent renewable energy resource‑based generating unit that opted to be classified as scheduled generating unit, necessary for the calculation of MAPE and PERC95 and for verification or validation of data, when necessary.
	Extended to include market offer data for VREs classified as scheduled generators. For must-dispatch units, forecast data is the relevant input. For VREs as scheduled, the relevant data is the offered quantity from market offers. Both data types are required for FPE calculation.
	
	
	
	

	4.1 Standards

	4.1.1
	Each must-dispatch generating unit shall comply with the following standards with respect to its mean absolute percentage error (MAPE) and percentile 95 of the forecasting error (Perc95) determined in accordance with Section 4.2 and calculated over the period specified in Section 4.1.2.

xxx
	Each must-dispatch generating unit shall comply with the following standards with respect to its mean absolute percentage error (MAPE) and percentile 95 of the forecasting error (Perc95) determined in accordance with Section 4.2 and calculated over the period specified in Section 4.1.2. Each intermittent renewable energy resource‑based generating unit that has opted to be classified as scheduled generating unit shall comply with the following standards with respect to its MPA and Perc95 based on the RTD schedule and Actual Dispatch determined in accordance with the applicable WESM Rules. 
	Standards provision extended to VREs that opted to be classified as scheduled generators. The same technology-based thresholds apply — Solar/Wind: MAPE < 18%, Perc95 < 30%; Run-of-River Hydro: MAPE < 9%, Perc95 < 30% — as the technologies are identical to those currently subject to FAS as must-dispatch units.
	
	
	
	

	4.2 Calculations
	4.2.4
	The projected quantity for each dispatch interval of a must-dispatch generating unit shall be calculated using the following formula: 

PQ(i,t) = (1/n) × (IL(i,t) + PO(i,t)) / 2

Where: 
xxx
PO(i,t) — projected output (in MW) of must-dispatch generating unit i for each dispatch interval t used in the scheduling process.
xxx
	The projected quantity for each dispatch interval of a must-dispatch generating unit shall be calculated using the following formula: 

PQ(i,t) = (1/n) × (IL(i,t) + PO(i,t)) / 2

Where: 
xxx
PO(i,t) — projected output (in MW) of must-dispatch generating unit i for each dispatch interval t used in the scheduling process. For an intermittent renewable energy resource‑based generating unit that has opted to be classified as scheduled generating unit, the projected output shall be equal to the RTD Schedule.
xxx
	Section 4.2.4 extended to cover VREs that opted to be classified as scheduled generators. The PQ formula is structurally identical, with the substitution of offered quantity in the form of projected output for the RTD schedule. 
	
	
	
	

	4.3 Exclusions and Other Basis for Recalculation
	4.3.1(a)
	(a) the dispatch target of the must-dispatch generating unit was restricted below its projected output.
	(a) the dispatch target of the must-dispatch generating unit or an intermittent renewable energy resource‑based generating unit that opted to be classified as scheduled generating unit was restricted below its projected output. For an intermittent renewable energy resource‑based generating unit that has opted to be classified as scheduled generating unit, the last tranche of the market offer shall be equal to its projected output.
	Exclusion extended to VREs that opted to be classified as scheduled generators. Reference to projected output supplemented with offered quantity in the form of projected output, consistent with the amended Projected Quantity definition.
	
	
	
	

	4.4 Monitoring, Reporting, and Review
	4.4.1
	The Enforcement and Compliance Office shall monitor the compliance of the Generation Company of each must-dispatch generating unit, calculate the MAPE and PERC95 and issue the Preliminary Forecast Accuracy Standards Reports including the data used in the calculation within 30 business days from the end of the calendar month of the covered monitoring period. For instance, the Preliminary Forecast Accuracy Standards Report for September billing period shall be issued not later than 30 October.
	The Enforcement and Compliance Office shall monitor the compliance of the Generation Company of each must-dispatch generating unit, or each intermittent renewable energy resource‑based generating unit that opted to be classified as scheduled generating unit, calculate the MAPE and PERC95 and issue the Preliminary Forecast Accuracy Standards Reports including the data used in the calculation within 30 business days from the end of the calendar month of the covered monitoring period. For instance, the Preliminary Forecast Accuracy Standards Report for September billing period shall be issued not later than 30 October.
	Monitoring obligation extended to VREs that opted to be classified as scheduled generators. Same 30-business-day timeline applies.
	
	
	
	

	4.4 Monitoring, Reporting, and Review
	4.4.4
	The Enforcement and Compliance Office shall issue the Final Forecast Accuracy Standards Report within seventy (70) business days from the end of the calendar month of the covered monitoring period regardless of whether a reply or confirmation is submitted by the concerned Generation Company or whether a recalculation of the results was performed for a particular must-dispatch generating unit.
	The Enforcement and Compliance Office shall issue the Final Forecast Accuracy Standards Report within seventy (70) business days from the end of the calendar month of the covered monitoring period regardless of whether a reply or confirmation is submitted by the concerned Generation Company or whether a recalculation of the results was performed for a particular must-dispatch generating unit or intermittent renewable energy resource‑based generating unit that opted to be classified as scheduled generating unit.
	Extended to VREs that opted to be classified as scheduled generators. Same 70-business-day deadline applies.
	
	
	
	

	4.4 Monitoring, Reporting, and Review 
	4.4.5
	The Enforcement and Compliance Office shall submit a consolidated monthly report to the PEM Board, the Compliance Committee, the ERC, and the DOE containing the status of the compliance of each must-dispatch generating unit to the forecast accuracy standards as of the most recent Billing Period based on the Final Forecast Accuracy Standards Report within the same timeline provided in Section 4.4.4 of this Manual.
	The Enforcement and Compliance Office shall submit a consolidated monthly report to the PEM Board, the Compliance Committee, the ERC, and the DOE containing the status of the compliance of each must-dispatch generating unit or each intermittent renewable energy resource‑based generating unit that opted to be classified as scheduled generating unit to the forecast accuracy standards as of the most recent Billing Period based on the Final Forecast Accuracy Standards Report within the same timeline provided in Section 4.4.4 of this Manual.
	Extended to VREs that opted to be classified as scheduled generators. Same monthly consolidated reporting obligation applies.
	
	
	
	

	4.5 Penalties and Sanctions
	4.5.2
	The Generation Company with must-dispatch generating unit that is in operation for less than a year and is found in breach of MAPE or PERC95, shall be: 
a) imposed a penalty in proportion to the number of months the must-dispatch generating unit is in operation during the covered monitoring year. For instance, the plant commenced operation on 26 March, the financial penalty to be imposed shall be in proportion to the nine (9) billing months over the twelve (12) month-period. 

b) exempted from liability, if it commences operation within three (3) months prior to the end of the covered monitoring year. 

A must-dispatch generating unit shall be considered in operation, for purposes of this Section, upon commencement of its operation or participation in the WESM either by virtue of the Final Certificate of Approval to Connect or the commercial operation registration in the WESM, whichever is applicable.
	The Generation Company with must-dispatch generating unit or intermittent renewable energy resource‑based generating unit that opted to be classified as scheduled generating unit that is in operation for less than a year and is found in breach of MAPE or PERC95, shall be: 
a) imposed a penalty in proportion to the number of months the must-dispatch generating unit or intermittent renewable energy resource‑based generating unit that opted to be classified as scheduled generating unit is in operation during the covered monitoring year. For instance, the plant commenced operation on 26 March, the financial penalty to be imposed shall be in proportion to the nine (9) billing months over the twelve (12) month-period. 
b) exempted from liability, if it commences operation within three (3) months prior to the end of the covered monitoring year. 

A must-dispatch generating unit or intermittent renewable energy resource‑based generating unit that opted to be classified as scheduled generating unit shall be considered in operation, for purposes of this Section, upon commencement of its operation or participation in the WESM either by virtue of the Final Certificate of Approval to Connect or the commercial operation registration in the WESM, whichever is applicable.
	Pro-rata penalty and new entrant exemption extended to VREs that opted to be classified as scheduled generators. A VRE electing scheduled status partway through a monitoring year receives pro-rated assessment; one commencing within three months of year-end is exempt.
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